Original VAG diagnostic and maintenance tool: [Xhorse Iscancar VAG MM-007](http://www.vvdishop.com/wholesale/xhorse-iscanner-vag-mm-007-diagnostic-tool.html)

the package:

packed well with two box, one paper box, and one plastic box



items includes Xhorse Iscancar VAG MM-007 main unit with an OBDII connector, and a USB cable used for connection to PC

the main unit

specification:


Voltage: 5V USB / 12V OBD  
LCD resolution: 320×240   
USB standard: USB2.0  
Working temperature: 0-60°C  
OBD line length: 1.5meters  
Power consumption: 80mA/12V



the port



the back, saying it supports J2534 SAE, J1850 PWM/VPW, ISO 14230-4 (KWP),  ISO 15764-4 (11 bit and 29 bit CAN), ISO 9141-2



Xhorse Iscancar VAG MM-007 main menu:

vag diagnostics

guide function


parameter refresh

special function


controller refresh

system setup

about iscancar




languages: only Chinese and English available




about Xhorse Iscancar VAG MM-007:


firmware version: 1.0.0

software version: 2.1.6





































VAG diagnostics...Here you go








systems that is supported



guide function :







parameter refresh:









 special function that Xhorse Iscancar VAG MM-007 can do:

change vin  
read pin  
immo switch  
adapt unit module  
key learning  
fix Audi RB4/RB8 not start  
transport mode  
sync dashboard time  
clear all DTCs  
gateway register

controller refresh:



firmware refresh

parameter refresh



system setup:

time and date  
log record  
display time  
set language  
scan QC code  
firmware update  
set WSC code  
TF card formate & create folders



Source:

<http://www.vvdishop.com/wholesale/xhorse-iscanner-vag-mm-007-diagnostic-tool.html>